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Section A 
Answer all questions in this section. 
1 Fig. 1 shows the rear derailleur gear on a cycle with a close up view of the gear cable. 
outer gear cable 
Fig. 1 
(a) Name the force that has been applied, when manufacturing the inner gear cable to keep the 
strands of cable in position. 
...............................................................................................................................................[1] 
(b) The outer gear cable has a nylon lining. 
Give two benefits of using the nylon lining. 
1 ................................................................................................................................................ 
2 ................................................................................................................................................ [2] 
(c) Explain why small radius bends should be avoided in the gear cable when it is attached to the cycle. ................................................................................................................................................... 
................................................................................................................................................... 
...............................................................................................................................................[2] 
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2 (a) Explain why steel is used for control cables on a cycle. 
................................................................................................................................................... 
................................................................................................................................................... 
...............................................................................................................................................[2] 
(b) State the force being used when a control cable is operated. 
...............................................................................................................................................[1] 
3 Hydraulic systems are now used for many applications rather than a control cable. 
State the force created in a hydraulic system. 
......................................................................................................................................................[1] 
4 Fig. 2 shows the speed control lever on a wood turning lathe. 
Slow 
Fast Fig. 2 
(a) Complete three of the labels to show the position of effort, load and fulcrum on the lever when it is used to change the speed of the lathe. [3] 
(b) State the order of lever used. 
...............................................................................................................................................[1] 
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5 Choose from the terms below to complete the table. 
bevel gear idler gear rack and pinion worm gear 
Requirement Method 
Transfer drive through 90° with no change in speed 
Provide a large reduction in speed in a small space 
Make driver and driven shafts rotate in the same direction 
[3] 
6 Fig. 3 shows a piece of rod with a square thread cut into it. 
3 6 
5 29 1Fig. 3 
State the pitch of the thread. 
......................................................................................................................................................[1] 
7 Fig. 4 shows two logic symbols with truth tables for each. 
AQ1A B Q1 
Q2 
B0 0 
Name.................... 
0 
1 
AB 
1 
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0 
Name.................... 
1 1Fig. 4 
(a) Write the name under each symbol. [2] 
(b) Complete the truth table. [2] 
5 
8 A catalogue describes two capacitors in the following way: 
• electrolytic capacitor 3300 μF 30 Vdc ± 20% 
• ceramic capacitor 100 pF 50 Vdc ± 10%. 
(a) Explain what is meant by 30 Vdc and 50 Vdc in the description of the capacitors. 
................................................................................................................................................... 
................................................................................................................................................... 
...............................................................................................................................................[2] 
(b) State why the electrolytic capacitor value is likely to vary more from its stated value than the 
ceramic capacitor. 
................................................................................................................................................... 
...............................................................................................................................................[1] 
9 Name the discrete component used with a capacitor to produce a delay in a circuit. 
......................................................................................................................................................[1] 
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10 Fig. 5 shows the initial design for a scaffold to give safe access while building work is carried out. 
X 
Y 
Fig. 5 
(a) (i) Name the type of structure used in scaffolding. 
.......................................................................................................................................[1] 
(ii) Draw on Fig. 5 three additional scaffolding poles to make the structure rigid and safe from collapse. [3] 
(iii) Explain the purpose of features X and Y at the base of the scaffold. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
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(iv) When scaffolding is designed, a factor of safety for the structure is considered. 
Explain what is meant by a factor of safety. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(b) Workers on a construction site have to wear ‘hard hats’ as shown in Fig. 6. 
Fig. 6 
(i) State the type of structure used in the hard hat. 
...................................................................................................................................... [1] 
(ii) Explain how the strength of the hard hat has been improved without adding any extra 
material. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
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(c) Fig. 7 shows the axes for a stress/strain graph for mild steel. 
The position of three features that will appear on the graph are marked. 
A 
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A – elastic limit B – upper yield point 
stress 
C – ultimate stress point 
strain 
Fig. 7 
(i) Draw the shape of the graph on Fig. 7. [3] 
(ii) Explain what is meant by ‘elastic limit’ on the graph. 
........................................................................................................................................... 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(d) Fig. 8a shows a folding clothes airer in the assembled position. 
Fig 8a Fig. 8b 
(i) Name the strengthening feature on the clothes airer shown in Fig. 8b. 
.......................................................................................................................................[1] 
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(ii) Give two reasons for using the type of strengthening feature shown in Fig. 8b. 
1 ........................................................................................................................................ 
........................................................................................................................................... 
2 ........................................................................................................................................ 
........................................................................................................................................... [2] 
(iii) The load carrying ability of each rail in the clothes airer is to be tested. 
Use sketches and notes on Fig. 9 to show how a dial gauge could be fixed to give a positive reading on the gauge when a load is added to the centre of the Ø6 rail. 
750 
6 ØØ12 
[3] Fig. 9 
Question 10 continues on the next page 
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(e) Fig. 10 shows two concrete pillars. 
7 kN 8 kN 
Ø200 
175 × 175 
pillar A pillar B 
Fig. 10 
Calculate which pillar is subject to the greatest stress when the loads are applied. 
Use the formula: stress = cross sectional force 
area 
................................................................................................................................................... 
................................................................................................................................................... 
................................................................................................................................................... 
...............................................................................................................................................[3] 
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11 Fig. 11 shows views of the chain drive on a cycle. 
10 sprockets 
jockey wheelschain 
2 chainrings 
Fig. 11 
(a) (i) Describe two functions of the jockey wheels in the chain drive. 
1 ........................................................................................................................................ 
........................................................................................................................................... 
2 ........................................................................................................................................ 
........................................................................................................................................... [2] 
(ii) Calculate the number of gear ratios that are available on the cycle. 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(iii) Name the factor, in addition to the number of sprockets and chainrings that will determine 
how far the cycle will travel for each rotation of the chainring. 
.......................................................................................................................................[1] 
(b) (i) Explain why a chain should be lubricated. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(ii) State why grease is not suitable for lubricating a chain. 
........................................................................................................................................... 
.......................................................................................................................................[1] © UCLES 2018 0445/43/M/J/18 [Turn over 
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(c) Fig. 12 shows three different types of bearing that can be used in a jockey wheel. 
© UCLES 2018 
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Fig. 12 
(i) Give one reason for using a rubber seal either side of the bearing in type R. 
........................................................................................................................................... 
.......................................................................................................................................[1] 
(ii) The outer bearing face in type R has four grooves cut into the surface; this is a common 
feature when using plain bearings. State the reason for the grooves. 
........................................................................................................................................... 
.......................................................................................................................................[1] 
(iii) Give one benefit for each of the bearing types used in S and T. 
Bearing S .......................................................................................................................... 
........................................................................................................................................... 
Bearing T ........................................................................................................................... 
........................................................................................................................................... [2] 
rubber seal 
grooves 
R plain bearing – ceramic 
S plain bearing – steel 
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(d) Fig. 13 shows the blade guide for a small bandsaw used for cutting timber. 
By turning handle A the guide can be raised or lowered to allow different thicknesses of timber to be cut. 
handle A 
visible part of mechanism 
blade guide 
saw table 
blade 
Fig. 13 
(i) Name the mechanism used to raise and lower the blade guide when handle A is turned. 
.......................................................................................................................................[2] 
(ii) State the conversion of motion which takes place when handle A is turned and the blade 
guide moves. 
...................................................... to ...................................................... [2] 
(iii) When the bandsaw is in use there are energy losses. 
Name two ways in which the energy from the motor can be lost when the machine is in use. 
1 ........................................................................................................................................ 
........................................................................................................................................... 
2 ........................................................................................................................................ 
........................................................................................................................................... [2] 
(iv) Describe how energy loss in a powered machine can be reduced. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
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(v) The guide fence for the saw is held securely in place by a cam lever shown in Fig. 14. 
unlocked 
locked position position cam profile 
Fig. 14 
Explain why cams are often used where frequent adjustment is necessary. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(e) Fig. 15 shows a compound pulley system. 
effort 
load 
Fig. 15 
(i) State the mechanical advantage of the pulley system. 
.......................................................................................................................................[1] 
(ii) Calculate the pulling force necessary to raise a load of 1.5 kN. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
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12 (a) Fig. 16 shows a push switch that could be either a PTM switch or a PTB switch, the two types 
are identical in size and colour. 
Fig. 16 
Use sketches and notes to explain how the switch action can be identified using a multimeter on a resistance setting. 
[3] 
(b) Fig. 17 shows three types of connecting wire that could be used to connect a switch to a 
circuit board. 
1 / 0.6 equipment wire 
1 / 0.6 non-insulated wire 
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7 / 0.2 equipment wire 
Fig. 17 
(i) State which type of connecting wire is the most suitable. 
.......................................................................................................................................[1] 
(ii) Give one reason for your choice of connecting wire. 
........................................................................................................................................... 
.......................................................................................................................................[1] 
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(iii) Use sketches and notes to describe four stages in soldering a connecting wire to a 
switch terminal. 
[4] 
(c) Fig. 18 shows a method of connecting a number of wires on a ribbon cable to a circuit board. 
10 way plug 
ribbon cable 
pins soldered to circuit board 
Fig. 18 
Give two advantages of using this method rather than soldering individual wires to the circuit board. 
1 ................................................................................................................................................ 
................................................................................................................................................... 
2 ................................................................................................................................................ 
................................................................................................................................................... [2] 
© UCLES 2018 
0445/43/M/J/18 
17 
(d) Fig. 19 shows a conveyor belt in a supermarket checkout area. 
The belt keeps going until an item of shopping blocks the path between the light source and an LDR on the other side of the conveyor belt. 
conveyor belt 
LDR LED Fig. 19 
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(i) Part of the operating circuit for the conveyor belt is shown in Fig. 20. 
+12 V 
R1 VR1 0 VVR2 
Y –X+ 
Fig. 20 
Calculate the value of R1 that should be used to allow the high intensity LED to draw a current of 40 mA. The forward voltage of the LED is 3.4 V. 
........................................................................................................................................... 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[3] 
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(ii) The operating circuit uses a CA3140 operational amplifier to compare the voltage from the LDR potential divider with a reference voltage provided by VR2 potential divider. Explain what is meant by ‘potential divider’. 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[2] 
(iii) Explain the operation of a voltage comparator. 
........................................................................................................................................... 
........................................................................................................................................... 
........................................................................................................................................... 
.......................................................................................................................................[3] 
(iv) State two ways of changing the sensitivity of the circuit. 
1 ........................................................................................................................................ 
2 ........................................................................................................................................ [2] 
(v) The high output of the CA3140 operational amplifier is +10 V with a maximum current of 
10 mA, which is not enough to operate the motor. Complete Fig. 21 to show a transistor circuit that will operate the relay to switch the motor on and off. 
+12 V 
–M + 
0 V© UCLES 2018 
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[3] Fig. 21 
(vi) Give one reason for using a relay to switch the motor on and off. 
........................................................................................................................................... 
.......................................................................................................................................[1] 
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